# Why go 2.5" pipe when the inlet of the muffler is barely 2.25"? Just wondering n/m

Posted by Jeff92se (92se) on June 17, 2002 at 19:46:06:

In Reply to: 2.5" custom catback to the muffler posted by Bret on June 17, 2002 at 18:39:43:

: it was $100 to put the muffler on and have the 2.5" catback made. Yes there is a difference in performance ;-)

Replys:

- So Jeff, what size did you go with? nm 808se (92SE) 02:27:59 6/18/2002 (0)
- are you just being difficult? :gotme: i went with 2.5"..why not? nm Chris91se (91se) 22:20:18 6/17/2002 (0)
- Why not? Which size is the best? n/m Aaron (92 SE Auto) 21:17:25 6/17/2002 (5)
  - Think about it..... Mike N (89 Gxe) 01:25:36 6/18/2002 (4)
    - Well, I think you are partially correct..... Mikey P (93 SE) 07:38:24 6/18/2002 (3)
      - yah, but it really depends on how the muffler was installed.. .. Mike N (89 Gxe) 15:26:49 6/18/2002 (2)
        - So, Mikey, how did you get the muffler installed? Smooth transition or a wall? n/m Aaron (92 SE Auto) 22:27:13 6/18/2002 (1)
          - something inbetween the two extreems :) n/m Mikey P (93 SE) 08:02:49 6/19/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : it was $100 to put the muffler on and have the 2.5" catback made. Yes there is a difference in performance ;-)