# I don't know of an ECU fail safe mode. Please enlighten me. n/m

Posted by Kaleb (Black '93 GXE 5spd) on June 16, 2002 at 15:03:03:

In Reply to: In preparation of my base map for the MoTeC, does the A/T computer still function normally when ECU goes into fail-safe mode? n/m posted by The Max on June 15, 2002 at 20:14:09:

: n/m

Replys:

- I.e. the crap that happens when the MAF isn't connected. limits RPm to 2000 or so. nm Matt (93SE) 13:15:31 6/17/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : n/m