# just remove the wire from the relay and ground it

Posted by «§»Craig B«§» (93 SE) on June 25, 2002 at 07:57:37:

In Reply to: Re: ECU Diagram posted by Victor A. Marques on June 24, 2002 at 22:49:05:

just pull the hood wire off the relay temporarily and ground it while you do whatever you need to for programming and then put it back into the relay when you're done

: I would like to thank all that helped me in installing my alarm, remote start, and keyless entry. I just have one final question and I feel Craig may be the one with the answer, I have it all working as I was informed now my question is how do i get into the programing mode since the hood pin is now connected for the remote start?

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: just pull the hood wire off the relay temporarily and ground it while you do whatever you need to for programming and then put it back into the relay when you're done : : I would like to thank all that helped me in installing my alarm, remote start, and keyless entry. I just have one final question and I feel Craig may be the one with the answer, I have it all working as I was informed now my question is how do i get into the programing mode since the hood pin is now connected for the remote start?