# yellow/green is the other

Posted by Craig B (93 SE) on June 17, 2002 at 13:45:05:

In Reply to: Re: When grounding VTC, is there only one wire (inside of the sheath) going to the solenoid? posted by Evil Yak on June 17, 2002 at 13:00:58:

yellow/green is teh one you want to ground
there should be those same two wires in the harness to each VTC solenoid

you only need to ground one because the wiring is all connected anyway
: there should be two...
: a red/black and something else
: don't ground the red/black... that's your ignition wire

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: yellow/green is teh one you want to ground : there should be those same two wires in the harness to each VTC solenoid : you only need to ground one because the wiring is all connected anyway : : there should be two... : : a red/black and something else : : don't ground the red/black... that's your ignition wire