# Any advice for 5th Gen muffler install?

Posted by 808se (92SE) on June 17, 2002 at 18:17:05:

I'll probably be getting it installed Friday. Any recommendations on piping size, resonator etc.? Any advice will help.

Replys:

- 2.5" custom catback to the muffler Bret (89SE) 18:39:43 6/17/2002 (9)
  - Why go 2.5" pipe when the inlet of the muffler is barely 2.25"? Just wondering n/m Jeff92se (92se) 19:46:06 6/17/2002 (8)
    - So Jeff, what size did you go with? nm 808se (92SE) 02:27:59 6/18/2002 (0)
    - are you just being difficult? :gotme: i went with 2.5"..why not? nm Chris91se (91se) 22:20:18 6/17/2002 (0)
    - Why not? Which size is the best? n/m Aaron (92 SE Auto) 21:17:25 6/17/2002 (5)
      - Think about it..... Mike N (89 Gxe) 01:25:36 6/18/2002 (4)
        - Well, I think you are partially correct..... Mikey P (93 SE) 07:38:24 6/18/2002 (3)
          - yah, but it really depends on how the muffler was installed.. .. Mike N (89 Gxe) 15:26:49 6/18/2002 (2)
            - So, Mikey, how did you get the muffler installed? Smooth transition or a wall? n/m Aaron (92 SE Auto) 22:27:13 6/18/2002 (1)
              - something inbetween the two extreems :) n/m Mikey P (93 SE) 08:02:49 6/19/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: I'll probably be getting it installed Friday. Any recommendations on piping size, resonator etc.? Any advice will help.