# yeah, but if you pop a vacuum line off -->

Posted by Matt K (89 SE 5spd) on June 23, 2002 at 22:05:19:

In Reply to: there's got to be a vacum port in the manifold u can disconnect and shoot it in there..nm posted by DanNY on June 23, 2002 at 22:02:39:

the car usually won't idle, you'll need somebody to sit in the car and rev it to keep it running. Not a big deal, but you do need the other person. You might need the other person anyway, I remember with my old motorcycle, it would die when you sprayed in carb cleaner if you didn't rev it up a bit. Either way ought to work fine.

Replys:

- well...the FPR doesn't really need the vacume during idle..nm DanNY (91SE) 07:48:47 6/24/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: the car usually won't idle, you'll need somebody to sit in the car and rev it to keep it running. Not a big deal, but you do need the other person. You might need the other person anyway, I remember with my old motorcycle, it would die when you sprayed in carb cleaner if you didn't rev it up a bit. Either way ought to work fine.