# Boot = trunk :p nm

Posted by James (92 SE auto) on June 17, 2002 at 20:27:49:

In Reply to: In the battery bay (relocating battery to the boot), attached to the motor with 2 thick steel bars to account for engine movement. n/m posted by The Max on June 17, 2002 at 20:26:50:

Replys:

- Yeah, what that Yank said 3#-) n/m The Max (92 J30 Maxima (turbo project underway)) 20:34:01 6/17/2002 (2)
  - Yanks live up north! We are Texans by God! n/m Bret (89SE) 01:20:21 6/18/2002 (1)
    - I know. That's why I said it 3#-) n/m The Max (92 J30 Maxima (turbo project underway)) 01:32:11 6/18/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments: