# ouch that sucks.....

Posted by Alex (90se5spd) on June 17, 2002 at 22:03:32:

In Reply to: Just replaced y-pipe with WSP y-pipe but now i have a ticking sound coming from the rear header...any suggestions??? (more) posted by kyle on June 17, 2002 at 21:54:33:

broken exhaust studs. goto the dealership and ask for the exhaust manifold to head studs. he should give you a bag labeled turbo. drill out the studs that are broken put in new ones. good luck, its a bitch of a job on the rear. remove ypipe, support motor with jack and block of wood via the oil pan, remove the rear engine mounts to get more room, curse and sware for starting this project. good luck

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: broken exhaust studs. goto the dealership and ask for the exhaust manifold to head studs. he should give you a bag labeled turbo. drill out the studs that are broken put in new ones. good luck, its a bitch of a job on the rear. remove ypipe, support motor with jack and block of wood via the oil pan, remove the rear engine mounts to get more room, curse and sware for starting this project. good luck