# Casting? No. 80-120 grit surface, yes. That's what I've done. I might also try the "Dimple" method at the injector nozzle. n/m

Posted by Kaleb (Black '93 GXE 5spd) on June 18, 2002 at 09:40:15:

In Reply to: T or F...you should keep some casting on the intake side.. posted by DanNY on June 18, 2002 at 08:08:11:

: to help atomize the fuel and air mixture?

: : http://www.4dsc.com/kaleb/enginehead/FrameSet.htm

: : -Kaleb

Replys:

- "Dimple method" ? n/m The Max (92 J30 Maxima (turbo project underway)) 10:22:18 6/18/2002 (4)
  - It's something like this.... Mikey P (93 SE) 10:34:25 6/18/2002 (3)
    - there's some good pics of it on endyn's website.. www.theoldone.com isn't it? nm Matt (93SE) 13:30:05 6/18/2002 (2)
      - very nice.... Mikey P (93 SE) 13:44:09 6/18/2002 (1)
        - Wow, that site kicks ass! *Add to Favorites* n/m Mikey P (93 SE) 13:49:26 6/18/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : to help atomize the fuel and air mixture? : : : <a href="http://www.4dsc.com/kaleb/enginehead/FrameSet.htm">http://www.4dsc.com/kaleb/enginehead/FrameSet.htm</a> : : : -Kaleb