# to drop the tranny you don't need to remove the ball joints...

Posted by Alex (90se5spd) on June 20, 2002 at 08:23:01:

In Reply to: Moron mechanics! ---> (venting) posted by John vdP on June 19, 2002 at 22:58:04:

all you need to do is remove the lower struts bolts to the hub, turn the steering wheeel all the way to the side and then wiggle the axel out, only necessary on the drivers side, the passenger side axle can stay in.

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: all you need to do is remove the lower struts bolts to the hub, turn the steering wheeel all the way to the side and then wiggle the axel out, only necessary on the drivers side, the passenger side axle can stay in.