# ATTN: Kaleb: When ECU has no crank angle sensor connected, it rev limits to 2000rpm. Perhaps you guys call it "Limp home mode?" n/m

Posted by The Max (92 J30 Maxima (turbo project underway)) on June 16, 2002 at 18:15:52:

n/m

Replys:

- How could it possibly know when 2,000 RPM is if it has no crank position sensor signal? --> Kaleb (Black '93 GXE 5spd) 18:36:11 6/16/2002 (1)
  - It works off limited parameters that "theoretically" result in 2000rpm operation. And yes, the FSM does say that, I just wanted reassurance. Thanks! 3#-) n/m The Max (92 J30 Maxima (turbo project underway)) 05:00:36 6/17/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: n/m