# Dumping the BOSE

Posted by mverse (90 GXE 92 SE spd) on June 15, 2002 at 19:09:49:

system in the 92SE. Just researching on the .org and came across this posting Click me Did anyone with an SE/BOSE system run into this issue. It basically advises to run new wiring to all the speakers ?!?! I read Craig's and Matt's page for the bypass..do you gents have any problems with it? Anybody here can relate to that?

Can someone confirm the front's are 6.5" I'm confused if it is 4x7 or 6.5

TIA
Abdul

Replys:

- you dont need to run new wires Craig B (93 SE) 19:23:55 6/15/2002 (1)
  - the fronts are around 4 inches, however you can prolly fit a shallow 8inch sub in there nm, Alex (90se5spd) 20:10:41 6/15/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: system in the 92SE. Just researching on the .org and came across this posting <a href="http://forums.maxima.org/showthread.php?s=95e764b1a47466b5a1c5858873a4562f&threadid=127820"> Click me </a> Did anyone with an SE/BOSE system run into this issue. It basically advises to run new wiring to all the speakers ?!?! I read Craig's and Matt's page for the bypass..do you gents have any problems with it? Anybody here can relate to that? : Can someone confirm the front's are 6.5" I'm confused if it is 4x7 or 6.5 : TIA : Abdul