# In preparation of my base map for the MoTeC, does the A/T computer still function normally when ECU goes into fail-safe mode? n/m

Posted by The Max (92 J30 Maxima (turbo project underway)) on June 15, 2002 at 20:14:09:

n/m

Replys:

- I assume it's totally unconnected since the ECU upgrade doesn't alter the shifting at all on my auto... Joel G. ('92 SE) 22:48:47 6/16/2002 (0)
- I don't know of an ECU fail safe mode. Please enlighten me. n/m Kaleb (Black '93 GXE 5spd) 15:03:03 6/16/2002 (1)
  - I.e. the crap that happens when the MAF isn't connected. limits RPm to 2000 or so. nm Matt (93SE) 13:15:31 6/17/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: n/m