# Why not? Which size is the best? n/m

Posted by Aaron (92 SE Auto) on June 17, 2002 at 21:17:25:

In Reply to: Why go 2.5" pipe when the inlet of the muffler is barely 2.25"? Just wondering n/m posted by Jeff92se on June 17, 2002 at 19:46:06:

: : it was $100 to put the muffler on and have the 2.5" catback made. Yes there is a difference in performance ;-)

Replys:

- Think about it..... Mike N (89 Gxe) 01:25:36 6/18/2002 (4)
  - Well, I think you are partially correct..... Mikey P (93 SE) 07:38:24 6/18/2002 (3)
    - yah, but it really depends on how the muffler was installed.. .. Mike N (89 Gxe) 15:26:49 6/18/2002 (2)
      - So, Mikey, how did you get the muffler installed? Smooth transition or a wall? n/m Aaron (92 SE Auto) 22:27:13 6/18/2002 (1)
        - something inbetween the two extreems :) n/m Mikey P (93 SE) 08:02:49 6/19/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : : it was $100 to put the muffler on and have the 2.5" catback made. Yes there is a difference in performance ;-)