# Is there a such thing as an "optimal" EGT reading during crusing and WOT???

Posted by DA-MAX (91 GXE) on July 04, 2002 at 02:01:25:

I've heard between 800-1000 is optimal for cruising speeds...but then at WOT, what is considered "optimal" or "regular"? we're getting 1300+/- at WOT...does that sound about right??

Replys:

- it all depends on the particular car, mods, and where the sensor is in the exhaust. best to tune on a dyno with a wideband O2 sensor and find what temps correspond to optimal A/F conditions. nm Matt (93SE) 10:13:24 7/05/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: I've heard between 800-1000 is optimal for cruising speeds...but then at WOT, what is considered "optimal" or "regular"? we're getting 1300+/- at WOT...does that sound about right??