# common sense (not to me): how much should spark plugs be torqued to? nm.

Posted by Maximax (93.VE.5SP) on July 03, 2002 at 18:25:15:

Replys:

- Replace them when the engine is cold. When you screw in and the gasket contacts, just give 1/4 and that's good enough. n/m Will (93 4dsc) 15:25:07 7/04/2002 (0)
- My 92 Maxima FSM says 14-22 ft-lbs. Yes, I finally have one. n/m Aaron (92 SE Auto) 23:39:25 7/03/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments: