# it all depends on the particular car, mods, and where the sensor is in the exhaust. best to tune on a dyno with a wideband O2 sensor and find what temps correspond to optimal A/F conditions. nm

Posted by Matt (93SE) on July 05, 2002 at 10:13:24:

In Reply to: Is there a such thing as an "optimal" EGT reading during crusing and WOT??? posted by DA-MAX on July 04, 2002 at 02:01:25:

: I've heard between 800-1000 is optimal for cruising speeds...but then at WOT, what is considered "optimal" or "regular"? we're getting 1300+/- at WOT...does that sound about right??

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : I've heard between 800-1000 is optimal for cruising speeds...but then at WOT, what is considered "optimal" or "regular"? we're getting 1300+/- at WOT...does that sound about right??