# Got my FSM now - it's the MAF sensor...

Posted by Uncle Pete (89 SE) on June 26, 2002 at 12:13:06:

In Reply to: Throttle Position Sensor failure I think... posted by Uncle Pete on June 26, 2002 at 04:52:03:

I got it the wrong way round. When the MAF sensor craps out the ECU guesses the settings using the throttle position sensor but caps revs to 2k.

Ah well, I was close.

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: I got it the wrong way round. When the MAF sensor craps out the ECU guesses the settings using the throttle position sensor but caps revs to 2k. : Ah well, I was close.