# Intrax guys you need to do this....

Posted by James (Didnt mess that one up!!) on July 07, 2002 at 23:09:14:

Vinyl tubing wrap the top and bottom coils of your springs. You can actually see there where the powdercoating is missing (rusted) where it'd been banged against the lower coil. I just did mine and whew made a huge difference in sound and squeakyness. Also put in new dustboots and bumpstops. =)

Replys:

- hmmm....now way am i touching my suspension again for awhile...lol nm Chris91se (91sae) 12:14:38 7/08/2002 (0)
- Eibach guys need it too in the rear. Where'd you get it? n/m Kaleb (Black '93 GXE 5spd) 23:53:06 7/07/2002 (2)
  - Good ole Home Depot...they have about 10 diff. sizes to choose from...nm James (92 SE auto) 23:56:27 7/07/2002 (1)
    - I guess this would be good for current or future Sprint guys also, thanks n/m MIKE (93VE) 10:35:25 7/08/2002 (0)
- Oh geez I give up... James (<---stupid) 23:11:37 7/07/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: <src img="http://images.cardomain.com/installs/140000-140999/140687_87_full.jpg"img> : Vinyl tubing wrap the top and bottom coils of your springs. You can actually see there where the powdercoating is missing (rusted) where it'd been banged against the lower coil. I just did mine and whew made a huge difference in sound and squeakyness. Also put in new dustboots and bumpstops. =)