# my car doesn't start with with engine continus button removed...nm

Posted by oE (91se) on June 28, 2002 at 09:57:30:

In Reply to: Attn: The Max..my findings with the ECCS..interestingly posted by abdul on June 28, 2002 at 09:53:50:

: enough, I checked the terminals for the engine cont relay under the hood..3 of the 4 poles had 12v DC. It looks like a short/open. I checked the readings on my other car, 90 GXE. Only 2 of them were hot, the way it should be. It looks like I have a hot wire crossing somehwere, or, some moronic hack went bad. To add, I checked the fuse panel in the car, and after removing the Engine cont 10A fuse, the car also starts !! but runs poorly, plugging the fuse back in while it is running, makes the car jumps overshoot RPM's and then back to base idle. I picked up the wiring diagram for the car and I'm going to trace the wires. It is going to be a pain, but, someone has got to do it. Thanks for your reply.

: Abdul

Replys:

- Your car is working the way it should be abdul (90 GXE 92 SE) 11:34:06 6/28/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : enough, I checked the terminals for the engine cont relay under the hood..3 of the 4 poles had 12v DC. It looks like a short/open. I checked the readings on my other car, 90 GXE. Only 2 of them were hot, the way it should be. It looks like I have a hot wire crossing somehwere, or, some moronic hack went bad. To add, I checked the fuse panel in the car, and after removing the Engine cont 10A fuse, the car also starts !! but runs poorly, plugging the fuse back in while it is running, makes the car jumps overshoot RPM's and then back to base idle. I picked up the wiring diagram for the car and I'm going to trace the wires. It is going to be a pain, but, someone has got to do it. Thanks for your reply. : : Abdul