# LOL...I was just about to ask if you had it! thanks man! :-) nm

Posted by DA-MAX (91 GXE) on July 03, 2002 at 16:31:05:

In Reply to: It's easy. 2 or 3 screws (you'll need a #3 phillips and some elbow grease though) and an e-clip on the end of the shaft. 5-10 min job to replace.. --> posted by Matt on July 03, 2002 at 16:29:03:

: And yes, it's already gone from my parts car. sold it a few weeks ago. sorry. :)

: : any ideas on the entire power valve assembly removal??? I think the actual actuator part has developed a leak...(evidence from the whinning noise it is making). looks like just unscrew and replace, any ideas

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : And yes, it's already gone from my parts car. sold it a few weeks ago. sorry. :) : : : any ideas on the entire power valve assembly removal??? I think the actual actuator part has developed a leak...(evidence from the whinning noise it is making). looks like just unscrew and replace, any ideas