# By bad on the VE oil pressure numbers, the switch info in EL-48 n/m

Posted by MIKE (93VE) on July 07, 2002 at 16:19:28:

In Reply to: actually, you're looking at VG data posted by «§» on July 07, 2002 at 15:56:05:

: I was looking through my FSM on friday but couldn't find any numbers for the oil pressure switch in the LC section. Where did you find it in the FSM?

: I found data on LC-4 for VG and LC-11 for VE in my 94FSM regarding what normal pressure should be
: at 3200, 53-65psi for VG like you said
: for VE: at 3000, 60-74psi

: not that it matters anyway, I just happened to be on the computer with the FSM next to me for some other stuff

: : It appears that our oil pressure switch is a NC switch with a 1.4-2.8psi pressure rating, so as stated before if we slowing started losing eng oil the light will not come on until the pressure drops below 2.8lbs that's scary. Also our oil pressure at idle should be 9psi and 53-65psi at 3,200 rpm

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : I was looking through my FSM on friday but couldn't find any numbers for the oil pressure switch in the LC section. Where did you find it in the FSM? : : I found data on LC-4 for VG and LC-11 for VE in my 94FSM regarding what normal pressure should be : : at 3200, 53-65psi for VG like you said : : for VE: at 3000, 60-74psi : : not that it matters anyway, I just happened to be on the computer with the FSM next to me for some other stuff : : : It appears that our oil pressure switch is a NC switch with a 1.4-2.8psi pressure rating, so as stated before if we slowing started losing eng oil the light will not come on until the pressure drops below 2.8lbs that's scary. Also our oil pressure at idle should be 9psi and 53-65psi at 3,200 rpm