# hmmm....now way am i touching my suspension again for awhile...lol nm

Posted by Chris91se (91sae) on July 08, 2002 at 12:14:38:

In Reply to: Intrax guys you need to do this.... posted by James on July 07, 2002 at 23:09:14:

:

: Vinyl tubing wrap the top and bottom coils of your springs. You can actually see there where the powdercoating is missing (rusted) where it'd been banged against the lower coil. I just did mine and whew made a huge difference in sound and squeakyness. Also put in new dustboots and bumpstops. =)

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : <src img="http://images.cardomain.com/installs/140000-140999/140687_87_full.jpg"img> : : Vinyl tubing wrap the top and bottom coils of your springs. You can actually see there where the powdercoating is missing (rusted) where it'd been banged against the lower coil. I just did mine and whew made a huge difference in sound and squeakyness. Also put in new dustboots and bumpstops. =)