# After doing a little FSM searching, more about the oil pressure switch >>>

Posted by MIKE (93VE) on July 07, 2002 at 15:22:36:

It appears that our oil pressure switch is a NC switch with a 1.4-2.8psi pressure rating, so as stated before if we slowing started losing eng oil the light will not come on until the pressure drops below 2.8lbs that's scary. Also our oil pressure at idle should be 9psi and 53-65psi at 3,200 rpm

Replys:

- actually, you're looking at VG data «§» (93 SE) 15:56:05 7/07/2002 (1)
  - By bad on the VE oil pressure numbers, the switch info in EL-48 n/m MIKE (93VE) 16:19:28 7/07/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: It appears that our oil pressure switch is a NC switch with a 1.4-2.8psi pressure rating, so as stated before if we slowing started losing eng oil the light will not come on until the pressure drops below 2.8lbs that's scary. Also our oil pressure at idle should be 9psi and 53-65psi at 3,200 rpm