# That is what happened to my injectors. Resistance was fine. Turned out that the tips were full of black gunk. n/m

Posted by Pervis Anathema ('91 SE) on July 08, 2003 at 18:24:01: In Reply to: correct on the work required.. the whole rail comes out at once, then you replace injectors as needed --> posted by Matt on July 08, 2003 at 10:49:45: : I didn't read the rest of the thread, but have you tried using any fuel system cleaners yet? they don't really "dry out", but what they will do is get gunky deposits in the tips and clog them up. they'll still read the proper resistance and sound like they're working, but they just won't spray. I ran into a problem with that last week on another guy's VG... time to clean them out and see what happens! Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: : I didn't read the rest of the thread, but have you tried using any fuel system cleaners yet? they don't really "dry out", but what they will do is get gunky deposits in the tips and clog them up. they'll still read the proper resistance and sound like they're working, but they just won't spray. I ran into a problem with that last week on another guy's VG... time to clean them out and see what happens!