# Correct

Posted by Tim (93se5sp) on July 15, 2003 at 06:39:47: In Reply to: Nasty... posted by Uncle Pete on July 15, 2003 at 06:06:04: It is important to get it level, but if it is out of square, the dooe will never operate properly. Just take some diagonal measurements and make sure they are equal. Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: It is important to get it level, but if it is out of square, the dooe will never operate properly. Just take some diagonal measurements and make sure they are equal.