# Warning.. 89-91 and 92-94 are different on the BOSE systems. nm

Posted by Matt (93SE) on September 04, 2002 at 00:09:01:

In Reply to: I have fronts and rears in excellent shape. E-mail me n/m posted by John vdP on September 03, 2002 at 22:41:38:

: .

Replys:

- I know h/u and CD connectors are different. What's different in the speakers? Connectors? mounting? n/m John vdP (93SE 5-sp) 21:02:35 9/04/2002 (0)
- Really? My car has the H.U. that looks like the '92+ single DIN. I do know that a 89-90 HU won't work. nm. delerium75 (91 GXE) 10:50:50 9/04/2002 (0)
- In what way are the different? I thought bose amps will fit 89 to 94 maximas. Mr. G (90 Max SE) 10:19:52 9/04/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : .