# Right, and further, with the VG, you're only draining 3 quarts out of 8, so it's a gradual process if you want it to be n/m

Posted by Bryan (91 SE, 92 SE) on September 05, 2002 at 07:19:28:

In Reply to: Well, some people thing that... posted by Uncle Pete on September 04, 2002 at 11:38:03:

: ...if the oil has been in there for ages then there can be deposits of crud lodged in various bits around the engine/gearbox. The idea is that the fresh oil could loosen up the crud and send it to all kinds of places in the engine/gearbox that you don't want it to go to.

: I'd just change it myself.

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : ...if the oil has been in there for ages then there can be deposits of crud lodged in various bits around the engine/gearbox. The idea is that the fresh oil could loosen up the crud and send it to all kinds of places in the engine/gearbox that you don't want it to go to. : : I'd just change it myself.