# haha, I gotta protect myself

Posted by «§» (93 SE) on September 03, 2002 at 23:41:48:

In Reply to: I recently replaced my first regulator and it's easy --> posted by Aaron on September 03, 2002 at 23:07:07:

yeah, 10mm socket will get your through most of it; only problem I've ever hard is on the screws holding the door panel pieces on (the hidden ones under the handle). They can be in pretty tight and if the screwdriver is too small, you can easily strip the screws.
With a #2 phillips, 10mm, 12mm, 14mm, and regular phillips, you can take apart nearly the whole interior of the car

I knew about the finger smashing thing, I just like to let the newbies find that part out the hard way j/k :)

: Little tip: Don't let the window fall and bash your
finger. Man, that hurt. Too bad Craig has a disclaimer on the write up or I will be filing some lawsuits. lol jk Craig.

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: yeah, 10mm socket will get your through most of it; only problem I've ever hard is on the screws holding the door panel pieces on (the hidden ones under the handle). They can be in pretty tight and if the screwdriver is too small, you can easily strip the screws. : With a #2 phillips, 10mm, 12mm, 14mm, and regular phillips, you can take apart nearly the whole interior of the car : I knew about the finger smashing thing, I just like to let the newbies find that part out the hard way j/k :) : : Little tip: Don't let the window fall and bash your : finger. Man, that hurt. Too bad Craig has a disclaimer on the write up or I will be filing some lawsuits. lol jk Craig.