# HEATER CORE FAILING YEARLY

Posted by THOMAS STEARNS (1978 FORD 250E VAN. 7.5L) on September 04, 2002 at 22:52:42:

I AM ON MY 8TH HEATER CORE.IT IS BEING OVER PRESSURIZED.RADIATOR CAP IS 14PSI. ALSO I GO THROUGH A RADIATOR EVERY 3 TO 4 YEARS.THIS IS A REBUILT MOTOR.COULD IT HAVE THE WRONG WATER PUMP? I NEED HELP!

Replys:

- 8th? Wow. Check the spec on the cap n/m Jeff92se (92se) 12:13:07 9/05/2002 (0)
- I saw 20/20 last night and they reviewed how bad those vans roll over with full weight when you snatch the wheel as hard as you can while going 75 mph. lol n/m Aaron (92 SE Auto) 10:05:22 9/05/2002 (2)
  - I hate 20/20, damn alarmists. nm Lordrandall (92se5-speed) 23:52:14 9/05/2002 (0)
  - Yes, the trick is getting to 75 :) n/m Bryan (91 SE, 92 SE) 20:35:20 9/05/2002 (0)
- Try this Ford Truck site>>>>>> MarkP (Maxima (had a Ford van)) 09:07:33 9/05/2002 (0)
- This is a Nissan Maxima board, not a Ford Van board.... Lordrandall (92se5-speed) 23:50:05 9/04/2002 (1)
  - ROTFLMAO dmontzmax (92 SE) 01:11:16 9/05/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: I AM ON MY 8TH HEATER CORE.IT IS BEING OVER PRESSURIZED.RADIATOR CAP IS 14PSI. ALSO I GO THROUGH A RADIATOR EVERY 3 TO 4 YEARS.THIS IS A REBUILT MOTOR.COULD IT HAVE THE WRONG WATER PUMP? I NEED HELP!