# Jeff - alignment specs with ST springs...

Posted by Jacob ('93 SE) on September 09, 2002 at 11:35:34:

They didn't align it because of my torn axle boot, but here's the specs they got off the car from when we re-assebled the suspension. Not too bad if you ask me...

Front:
Camber: L: -.70 R: -.50
Caster: L: +1.3 R: +1.00
Toe: L: +.04 R: +.04

Rear:
Camber: L: -.80 R: -.80
Toe: L: +.12 R: -.04

Definitely need some adjustments but it's not as crazy as I was expecting. With my rear toe settings, I should be able to make some pretty crazy LH turns.

-Jacob

Replys:

- I just had mine aligned (I have Eibachs)... RosenKen (93 SE 5spd) 18:03:29 9/09/2002 (2)
  - Here's a good pic, you can see there's not much front camber at all... RosenKen (93 SE 5spd) 18:45:02 9/09/2002 (1)
    - Wow, how bout we start the "Black VE with 5th gen spokes, Kuhmos, and Eibachs" club...nm blackandwhite (93 VE 5spd) 12:23:50 9/13/2002 (0)
- Nice. I wonder why mine is so fubar'd with just the Eibachs n/m Jeff92se (92se) 12:01:03 9/09/2002 (7)
  - Wreck? bent control arms? worn bushings? how far off is it? nm Matt (93SE) 13:08:52 9/09/2002 (4)
    - No bad wrecks. Nothing is bent up front. Rears are like -0.9(not bad) but one of the fronts is -1.1(not horrendous but tire wear is noticable)-> Jeff92se (92se) 13:50:58 9/09/2002 (3)
      - I had it too, until I changed out the ball joints..since then, it's been cool. blackandwhite (93 VE 5spd) 12:26:08 9/13/2002 (0)
      - Mine are close to that also, but that's easy to fix. unbolt the two bolts on the spindle, yank that sumbitch out some, then bolt it back together. there's a degree of play in the bolts. nm Matt (93SE) 01:01:29 9/10/2002 (0)
      - I have the exact same issue, same suspension/tire setup as Jeff... Jonny (94se 5spd) 16:04:51 9/09/2002 (0)
  - Because your upper strut mount insulators are worn out? n/m Kaleb (Black '93 GXE) 12:04:01 9/09/2002 (1)
    - They seemed okay then. Why would the alignment necessarily go neg when they are bad? And how can you tell if they are bad n/m Jeff92se (92se) 12:08:59 9/09/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: They didn't align it because of my torn axle boot, but here's the specs they got off the car from when we re-assebled the suspension. Not too bad if you ask me... : Front: : Camber: L: -.70 R: -.50 : Caster: L: +1.3 R: +1.00 : Toe: L: +.04 R: +.04 : Rear: : Camber: L: -.80 R: -.80 : Toe: L: +.12 R: -.04 : Definitely need some adjustments but it's not as crazy as I was expecting. With my rear toe settings, I should be able to make some pretty crazy LH turns. : -Jacob