# Your VE engine does not have a distributor.. I just used an enigne foam cleaner but I make sure that I wrap up the coils, power transistor and just about anything you don't want to get wet. Then use a very fine spray nozzle to hose it down. nm

Posted by G3Max (92 SE Auto (out of commission needs a ring job) & 92 SE 5 speed) on September 07, 2002 at 10:49:21:

In Reply to: What parts of the VE should be covered/taped up before blasting it with engine cleaner and the hose? obviously not the distributor but is there anything i should be careful with? n/m posted by mentat on September 07, 2002 at 09:33:41:

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments: