# Because your upper strut mount insulators are worn out? n/m

Posted by Kaleb (Black '93 GXE) on September 09, 2002 at 12:04:01:

In Reply to: Nice. I wonder why mine is so fubar'd with just the Eibachs n/m posted by Jeff92se on September 09, 2002 at 12:01:03:

: : They didn't align it because of my torn axle boot, but here's the specs they got off the car from when we re-assebled the suspension. Not too bad if you ask me...

: : Front:
: : Camber: L: -.70 R: -.50
: : Caster: L: +1.3 R: +1.00
: : Toe: L: +.04 R: +.04

: : Rear:
: : Camber: L: -.80 R: -.80
: : Toe: L: +.12 R: -.04

: : Definitely need some adjustments but it's not as crazy as I was expecting. With my rear toe settings, I should be able to make some pretty crazy LH turns.

: : -Jacob

Replys:

- They seemed okay then. Why would the alignment necessarily go neg when they are bad? And how can you tell if they are bad n/m Jeff92se (92se) 12:08:59 9/09/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : : They didn't align it because of my torn axle boot, but here's the specs they got off the car from when we re-assebled the suspension. Not too bad if you ask me... : : : Front: : : : Camber: L: -.70 R: -.50 : : : Caster: L: +1.3 R: +1.00 : : : Toe: L: +.04 R: +.04 : : : Rear: : : : Camber: L: -.80 R: -.80 : : : Toe: L: +.12 R: -.04 : : : Definitely need some adjustments but it's not as crazy as I was expecting. With my rear toe settings, I should be able to make some pretty crazy LH turns. : : : -Jacob