# brembos...arrived...quick ques...>

Posted by oE (91se) on September 03, 2002 at 22:32:50:

what exactly are the break in periods for new rotors? should I use the pads currently on there...they're still good? I heard from Matt93se that the best way was to use the old pads to break in the new rotors...please correct me if I'm wrong...and tell me anything else you feel like saying...;D

Replys:

- i did pads/rotors together...the rotors should have come with a detailed sheet of the break-in periord...just follow that nm Chris91se (91se) 07:13:37 9/04/2002 (1)
  - they did but I knew there was something about using old pads....so its kewl to use new ones? nm oE (91se) 08:04:37 9/04/2002 (0)
- Re: brembos...arrived...quick ques...> James (2 VE's) 23:29:49 9/03/2002 (0)
- Matt's right --> John vdP (93SE 5-sp) 22:46:05 9/03/2002 (2)
  - break in is closer to 3-400 miles on new rotors. pads are usually okay out of the box, except for some organic brands. nm Matt (93SE) 23:52:54 9/03/2002 (1)
    - CF and Carbon Kevlar pads have very strict bedding procedures as well. nm Jacob ('93 SE) 12:16:25 9/04/2002 (0)
- I would like to say--> Matt K (89 SE 5spd ) 22:35:32 9/03/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: what exactly are the break in periods for new rotors? should I use the pads currently on there...they're still good? I heard from Matt93se that the best way was to use the old pads to break in the new rotors...please correct me if I'm wrong...and tell me anything else you feel like saying...;D