# Easy, --->

Posted by RHD MAX (93 SE) on September 11, 2002 at 13:44:47:

In Reply to: how do i change the boot over the axle posted by jon on September 11, 2002 at 13:12:16:

Wheel off, big axle nut off, swing the hub assy away, pull the whole half shaft out of the tranny. (after draining of course. cut old boot off, knock CV joint off the shaft. Clean and relube, install new boot, put CV joint back on shaft, making sure the split ring seats in the groove. Place half shaft back in tranny, again making sure the split ring pops into place... refill with ATF (refer to Owners manual or FSM for proper fluid level, and how to check it..... then reverse order for the other shit. caliper, axle nut, wheel!

Replys:

- also remove the caliper and disc to make things easy--> RHD MAX (93 SE) 18:08:10 9/11/2002 (0)
- Add 2 hours of cleaning after making a huge greasy mess! hehe n/m Jeff92se (92se) 13:49:04 9/11/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: Wheel off, big axle nut off, swing the hub assy away, pull the whole half shaft out of the tranny. (after draining of course. cut old boot off, knock CV joint off the shaft. Clean and relube, install new boot, put CV joint back on shaft, making sure the split ring seats in the groove. Place half shaft back in tranny, again making sure the split ring pops into place... refill with ATF (refer to Owners manual or FSM for proper fluid level, and how to check it..... then reverse order for the other shit. caliper, axle nut, wheel!