# So why did you run all your grounds to the head? n/m

Posted by Jeff92se (92se) on September 19, 2003 at 15:28:54: In Reply to: 8 awg minimum. 4 would be best, but sometimes it's hard to do. --> posted by Matt on September 19, 2003 at 15:01:50: : that's one of those things I forgot to mention.. : should probably run an additional 4 awg wire to the block. don't mess with the frame. run it to a spot on the block, then reference all the other grounds on the engine to there. : would probably be good to ground the case of the alternator better too... Replys: Block/head, what's the difference?! :) --> Matt (93SE) 15:42:17 9/19/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: : that's one of those things I forgot to mention.. : : should probably run an additional 4 awg wire to the block. don't mess with the frame. run it to a spot on the block, then reference all the other grounds on the engine to there. : : would probably be good to ground the case of the alternator better too...