# Or a snap-on ratchet with a swivel head on it. works great. :) nm

Posted by Matt (93SE) on September 20, 2003 at 20:08:17: In Reply to: Hardest part is 1) Remove axle nut and 2) Removing 3 12mmX60mm hex bolts that hold axle into bearing bracket. You need long open end wrench or offset wrench (Wal-mart) n/m posted by Kaleb on September 20, 2003 at 11:57:32: : : n/m Replys: yep, gotta luv that swivel head. I've removed axels twice with it. prefect. n/m unsigned (92SE/89GXE) 09:16:42 9/21/2003 (1) Yup.. but now I can't find it. grrrrr. still have my 3/8" one, but not my 1/4". matt (93SE) 09:51:19 9/21/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: : : n/m