# What I might do is >>>>

Posted by The Max (92 J30 Maxima (turbo project nearing completion)) on September 15, 2003 at 18:12:58: In Reply to: with ~500hp, he's going to need all the engine mount he can get. Tony--> posted by Matt on September 15, 2003 at 14:47:31: have a steel plate welded to the underside of it like you're planning, but I have to say though, yours was rusted right through! That's why I had mine sandblasted and powdercoated again (surface rust). Replys: it was raining when it happened.. most of that rust was because it got wet after it cracked --> Matt (93SE) 08:24:21 9/16/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: have a steel plate welded to the underside of it like you're planning, but I have to say though, yours was rusted right through! That's why I had mine sandblasted and powdercoated again (surface rust).