# inner tie rod servicable?

Posted by denga (92gxe) on September 15, 2003 at 10:49:47: The bellow boot on passenger side broke. I am wondering if the inner tie rod has any bearings in it that need grease to keep working? i can't find any info on clinton and haynes manuals. Should i change it or just the boot itself? Has anyone had this experience before? i can't see any grease in the boot. Is the inner tie rod just a rod or has it some kind of greasable joint? thanks in advance. denga Replys: It's got a ball/socket joint in it. when you change the old boot, clean and grease the joint and you should be okay --> Matt (93SE) 10:56:41 9/15/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: The bellow boot on passenger side broke. : I am wondering if the inner tie rod has any bearings in it that need grease to keep working? : i can't find any info on clinton and haynes manuals. : Should i change it or just the boot itself? : Has anyone had this experience before? : i can't see any grease in the boot. : Is the inner tie rod just a rod or has it some kind of greasable joint? : thanks in advance. : denga