# What size is that axle nut anyways? n/m

Posted by Ant (Red '92 SE) on September 21, 2003 at 19:24:34: In Reply to: Hardest part is 1) Remove axle nut and 2) Removing 3 12mmX60mm hex bolts that hold axle into bearing bracket. You need long open end wrench or offset wrench (Wal-mart) n/m posted by Kaleb on September 20, 2003 at 11:57:32: : : n/m Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: : : n/m