# 8 awg minimum. 4 would be best, but sometimes it's hard to do. -->

Posted by Matt (93SE) on September 19, 2003 at 15:01:50: In Reply to: You think using a 8awg for the battery ground is good enough because it's an add on? n/m posted by Jeff92se on September 19, 2003 at 14:49:35: that's one of those things I forgot to mention.. should probably run an additional 4 awg wire to the block. don't mess with the frame. run it to a spot on the block, then reference all the other grounds on the engine to there. would probably be good to ground the case of the alternator better too... Replys: So why did you run all your grounds to the head? n/m Jeff92se (92se) 15:28:54 9/19/2003 (1) Block/head, what's the difference?! :) --> Matt (93SE) 15:42:17 9/19/2003 (0) So maybe in my case... Jacob ('03 WRX) 15:16:54 9/19/2003 (3) Personally, I wouldn't mess with the body ground, but it definitely can't hurt. nm Matt (93SE) 15:27:10 9/19/2003 (2) On my car.. Jacob ('03 WRX) 16:18:48 9/19/2003 (1) gotcha. nm Matt (93SE) 16:19:59 9/19/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: that's one of those things I forgot to mention.. : should probably run an additional 4 awg wire to the block. don't mess with the frame. run it to a spot on the block, then reference all the other grounds on the engine to there. : would probably be good to ground the case of the alternator better too...