# with ~500hp, he's going to need all the engine mount he can get. Tony-->

Posted by Matt (93SE) on September 15, 2003 at 14:47:31: In Reply to: WOW...that looks beautiful...question...why not shave a bit of the engine mount where the fitting is? nm posted by oE on September 15, 2003 at 11:43:59: I'm pretty sure we talked about this before, but make sure the crossmember underneath the car had been reinforced. do I need to remind you of why? :) http://www.mattblehm.com/pics/car/crossmember/ Replys: What I might do is >>>> The Max (92 J30 Maxima (turbo project nearing completion)) 18:12:58 9/15/2003 (1) it was raining when it happened.. most of that rust was because it got wet after it cracked --> Matt (93SE) 08:24:21 9/16/2003 (0) What did you use to reinforce yours? n/m Pervis Anathema ('91 SE) 15:04:04 9/15/2003 (1) nothing yet. I'm goign to buy another one and have some steel strips welded onto it for more strength. nm Matt (93SE) 15:08:13 9/15/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: I'm pretty sure we talked about this before, but make sure the crossmember underneath the car had been reinforced. do I need to remind you of why? :) : http://www.mattblehm.com/pics/car/crossmember/