# Hardest part is 1) Remove axle nut and 2) Removing 3 12mmX60mm hex bolts that hold axle into bearing bracket. You need long open end wrench or offset wrench (Wal-mart) n/m

Posted by Kaleb (Black '93 GXE 5spd) on September 20, 2003 at 11:57:32: In Reply to: How difficult is it to change out a passender side CV axle with auto and abs? Anything specific I gotta look out for?n/m posted by Ant on September 20, 2003 at 10:45:47: : n/m Replys: What size is that axle nut anyways? n/m Ant (Red '92 SE) 19:24:34 9/21/2003 (0) Or a snap-on ratchet with a swivel head on it. works great. :) nm Matt (93SE) 20:08:17 9/20/2003 (2) yep, gotta luv that swivel head. I've removed axels twice with it. prefect. n/m unsigned (92SE/89GXE) 09:16:42 9/21/2003 (1) Yup.. but now I can't find it. grrrrr. still have my 3/8" one, but not my 1/4". matt (93SE) 09:51:19 9/21/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: : n/m