# i just picked up the stuff at a local race shop -->

Posted by Matt (93SE) on September 22, 2003 at 23:42:50: In Reply to: Awesome..... posted by 8ball on September 22, 2003 at 23:01:37: take the calipers in there as well as your stainless lines. chop the banjo fitting off the end, and just start grabbing fittings out of the box until you have it working right. I ended up using a 1/8" NPT fitting with a 90deg bend to an AN fitting that the brake line connected to (the blue guy in the pic below). the goodridge SS are a standard size, and the screw-on fittings at the parts store will go right on. Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: take the calipers in there as well as your stainless lines. chop the banjo fitting off the end, and just start grabbing fittings out of the box until you have it working right. : I ended up using a 1/8" NPT fitting with a 90deg bend to an AN fitting that the brake line connected to (the blue guy in the pic below). the goodridge SS are a standard size, and the screw-on fittings at the parts store will go right on. : <img src=http://www.mattblehm.com/pics/car/brakes/24.jpg>