# Exactly what I did. Only I had to cut them a little shorter to fit it in my battery box in the trunk. n/m

Posted by The Max (92 J30 Maxima (turbo project nearing completion)) on September 27, 2003 at 19:15:00: In Reply to: Rather than use a spacer, I just used a tap/die set to extend the threads on the battery hold-down bar. n/m posted by Kaleb on September 27, 2003 at 17:42:38: : : 750CCAs and a 3yr full replacement warienty, hard to beat. The spacer lets it fit pretty well but the ground wire was a bit of a stretch... good thing I got my blehm co. ground kit today! Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: : : 750CCAs and a 3yr full replacement warienty, hard to beat. The spacer lets it fit pretty well but the ground wire was a bit of a stretch... good thing I got my blehm co. ground kit today!