# Ohhhh, so you're saying the y pipe is still bolted to the manifolds, but all other pipe is welded? nm

Posted by Matt (93SE) on October 02, 2003 at 23:09:37: In Reply to: I think how they did it was to let the y-pipe.. posted by SeaMAX on October 02, 2003 at 22:57:11: : or parts of it hang down hang down on stands or it might have been on the RSB while the flex section was bent and work their way back. I see no flanges. Replys: Exactly, that's the way my exhaust is MIKEq (93VE) 04:35:47 10/03/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: : or parts of it hang down hang down on stands or it might have been on the RSB while the flex section was bent and work their way back. I see no flanges.