# I also notice that on Ash's drawing

Posted by MIKE (93VE) on October 08, 2003 at 09:31:23: In Reply to: More notes. Ash used 4144 cold rolled steel and his brackets posted by Jeff92se on October 08, 2003 at 01:03:19: His dimensions wasn't completely square, his hole dimensions were different on both sides. From talking to Keith he's planning on using 303 SS, if aluminum was needed I would suggest 6061 T-6 I honeslty do not know the metalurgy of the different kind of metals, which one is better, etc. so I can't input much there. I pretty much would have left it up to the machinist. Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: His dimensions wasn't completely square, his hole dimensions were different on both sides. From talking to Keith he's planning on using 303 SS, if aluminum was needed I would suggest 6061 T-6 : I honeslty do not know the metalurgy of the different kind of metals, which one is better, etc. so I can't input much there. : I pretty much would have left it up to the machinist.