# Keep chuging along don't stop the more the merrier

Posted by MIKE (93VE) on October 06, 2003 at 16:15:58: In Reply to: Whatever that Z guy used. 10mm aka 3/8" or whatever posted by Jeff92se on October 06, 2003 at 15:34:24: The biggest problem for me was also drilling and spacing the 4 holes correctly. Holes too wide will allow the bracket to flop around, and the spacing of the holes dictate the caliper to rotor clearance. Fabricating the basic shape of the bracket was pretty straight forward. Replys: Ok. I got lucky. My dad has a drill press and a bit that was the exact Jeff92se (92se) 16:37:21 10/06/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: The biggest problem for me was also drilling and spacing the 4 holes correctly. Holes too wide will allow the bracket to flop around, and the spacing of the holes dictate the caliper to rotor clearance. : Fabricating the basic shape of the bracket was pretty straight forward.