# yeah, but its in the pan, right? this way its nice fresh oil straight to each cylinder. n/m

Posted by mentat (93se 5spd) on September 17, 2004 at 10:54:12: In Reply to: If he's running the engine, isn't there oil in there already? n/m posted by Jeff92se on September 17, 2004 at 10:02:48: : : the last thing you want to do is get a ton of rust on the cylinder walls. coating the top of the piston in oil and splashing it around in there should help keep it from really scarring anything up. : : I would highly suggest using a rubber hose and sucking any water you can out. once you've got that much out, you can likely just put the plugs back in and fire it up. the rest of the water will burn off. Replys: Not sure how much H20 could work it's way past the cylinder rings Jeff92se (92se) 11:18:54 9/17/2004 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: : : the last thing you want to do is get a ton of rust on the cylinder walls. coating the top of the piston in oil and splashing it around in there should help keep it from really scarring anything up. : : : I would highly suggest using a rubber hose and sucking any water you can out. once you've got that much out, you can likely just put the plugs back in and fire it up. the rest of the water will burn off.