# the bushings don't have the same outer race as the front control arm bushings -->

Posted by Matt (93SE) on September 08, 2004 at 14:02:39: In Reply to: Parallel Link Bushing Replacement question posted by MrGone on September 08, 2004 at 14:00:24: so you can usually just press them out with a pair of large sockets and a bench vise.. use one on the outside of the bar, then another to push the old bushing out from the other side. Replys: IBjeffymakesfunofme MrGone (92se) 14:11:58 9/08/2004 (1) pulley puller dude. nm Matt (93SE) 14:15:19 9/08/2004 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: so you can usually just press them out with a pair of large sockets and a bench vise.. use one on the outside of the bar, then another to push the old bushing out from the other side.